Request-Line: INVITE sip:03271485@x.x.x.x:50666 SIP/2.0

Record-Route: sip:y.y.y.y;lr=on

Via: SIP/2.0/UDP y.y.y.y;branch=z9hG4bKce48.40d19c96.0

Via: SIP/2.0/UDP z.z.z.z:45669;rport=45669;

branch=z9hG4bKPj28UvXKngB3PjBBmoyrTFZXoeNcVx4oIm

Max-Forwards: 16

From: sip:511@y.y.y.y;tag=-4TgMXfcfaV0Cj5VnCIxOkL1QmHji8PL

To: sip:411@y.y.y.y

Contact: sip:80945273@z.z.z.z:45669

Call-ID: bpOWizGe-SHsjIZXSLKptnnDBVi7dMnY

CSeq: 3687 INVITE

Allow: SUBSCRIBE, NOTIFY, PRACK, INVITE, ACK, BYE, CANCEL, UPDATE, MESSAGE, REFER

Supported: 100rel, replaces, norefersub, gruu

User-Agent: sipsimple 1.3.0

Content-Type: application/sdp

Content-Length:297

v=0

o=- 3612147894 3612147894 IN IP4 z.z.z.z

s=sipsimple 1.3.0

c=IN IP4 z.z.z.z

t= 0 0

m=message 2855 TCP/TLS/MSRP \*

a=path:msrps://z.z.z.z:2855/7ad200ec7137e5ed1a58;tcp

a=accept-types:message/cpim text/\* application/im-iscomposing+xml

a=accept-wrapped-types:\*

a=setup:active

Status-Line: SIP/2.0 500 Internal Server Error

Via: SIP/2.0/UDP y.y.y.y;received=y.y.y.y;branch=z9hG4bKce48.40d19c96

Via: SIP/2.0/UDP z.z.z.z:45669;rport=45669 branch=z9hG4bKPj28UvXKngB3PjBBmoyrTFZXoeNcVx4oIm

Record-Route: <sip:y.y.y.y;lr>

Call-ID: bpOWizGe-SHsjIZXSLKptnnDBVi7dMnY

From: sip:511@y.y.y.y;tag=-4TgMXfcfaV0Cj5VnCIxOkL1QmHji8PL

To: sip:411@y.y.y.y;tag=XKuUttlVFnfBakd5ATHkw9nhmIEOtCL2

CSeq:3687 INVITE

Server: sipsimple 1.3.0

AllowSUBSCRIBE, NOTIFY, PRACK, INVITE, ACK, BYE, CANCEL, UPDATE, MESSAGE, REFER

Reason: SIP ;text=\"media stream failed to start\" ;cause=500

Content-Length: 0